# Class CIM_AGPVideoDisplayController
extends CIM_DisplayController

Capabilities and management of an AGPVideoDisplayController.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Controller
|
+--CIM_DisplayController
|
+--CIM_AGPVideoDisplayController

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of an AGPVideoDisplayController.
Experimental | boolean | true
UMLPackagePath | string | CIM::Device::Controller
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AddressingMode | uint16 |
Description | string | An integer enumeration indicating the addressing mode of the graphics Controller.
ModelCorrespondence | string | CIM_AGPVideoDisplayController.OtherAddressingMode
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, Other, Sideband, Pipeline
AGPSpecificationVersionConformance | string |
Description | string | A string containing the AGP specification version to which this graphics Controller conforms.
DataTransferRate | uint16 |
Description | string | An integer enumeration indicating the data transfer rate of the graphics Controller.
ModelCorrespondence | string | CIM_AGPVideoDisplayController.OtherDataTransferRate
ValueMap | string | 0, 1, 2, 3, 4, 5
Values | string | Unknown, Other, 1X, 2X, 4X, 8X
GraphicsApertureSize | uint32 |
Description | string | Size of the graphics aperture in KB.
PUnit | string | byte * 2^10
Units | string | KiloBytes
LocalBusWidth | uint32 |
Description | string | Width of the internal bus in the graphics Controller, in bits.
PUnit | string | bit
Units | string | Bits
MaximumAGPCommandQueuePath | uint32 |
Description | string | The maximum number of AGP Transaction requests that the master (AGP Graphics Controller) is allowed to enqueue into the target.
MaxNumberOfPipelinedAGPTransactions | uint32 |
Description | string | The number of AGP Transaction that the core logic (chipset) can accept into its transaction request queue from the Controller.
NonlocalVideoMemorySize | uint32 |
Description | string | Size of the non-local video memory in KB.
PUnit | string | byte * 2^10
Units | string | KiloBytes
OtherAddressingMode | string |
Description | string | A string describing the addressing mode when the instance's AddressingMode property is 1 ("Other").
ModelCorrespondence | string | CIM_AGPVideoDisplayController.AddressingMode
OtherDataTransferRate | string |
Description | string | A string describing the data transfer rate when the instance's DataTransferRate property is 1 ("Other").
ModelCorrespondence | string | CIM_AGPVideoDisplayController.DataTransferRate
OtherUsageModel | string |
Description | string | A string describing the usage mode when the instance's UsageModel property is 1 ("Other").
ModelCorrespondence | string | CIM_AGPVideoDisplayController.UsageModel
UsageModel | uint16 |
Description | string | An integer enumeration indicating the usage model of the graphics Controller. Usage model indicates how the Controller does manipulations of graphics surfaces, textures, etc. in memory. DMA indicates that the graphics Controller brings structures from the system memory to its local memory to perform needed manipulations or renderings. Execute specifies that the graphics Controller can directly access a specified region in main memory (called the graphics aperture) using GART - Graphics Aperture Remapping Table. It then performs manipulations in that range as if that whole graphics aperture were part of its local memory. A value of "Both" DMA and Execute models may also be specified.
ModelCorrespondence | string | CIM_AGPVideoDisplayController.OtherUsageModel
ValueMap | string | 0, 1, 2, 3, 4
Values | string | Unknown, Other, Execute, DMA, Both

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AllocationState | string | CIM_LogicalDevice
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_DisplayController
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxMemorySupported | uint32 | CIM_DisplayController
MaxNumberControlled | uint32 | CIM_Controller
MaxQuiesceTime | uint64 | CIM_LogicalDevice
Name | string | CIM_ManagedSystemElement
NumberOfVideoPages | uint32 | CIM_DisplayController
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherVideoArchitecture | string | CIM_DisplayController
OtherVideoMemoryType | string | CIM_DisplayController
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
ProtocolDescription | string | CIM_Controller
ProtocolSupported | uint16 | CIM_Controller
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastReset | datetime | CIM_Controller
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
VideoArchitecture | uint16 | CIM_DisplayController
VideoMemoryType | uint16 | CIM_DisplayController
VideoProcessor | string | CIM_DisplayController
AcceleratorCapabilities | uint16[] | CIM_DisplayController
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
CapabilityDescriptions | string[] | CIM_DisplayController
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice