# Class CIM_DisplayController
extends CIM_Controller

Capabilities and management of the DisplayController.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Controller
|
+--CIM_DisplayController

## Direct Known Subclasses

CIM_AGPVideoDisplayController

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of the DisplayController.
UMLPackagePath | string | CIM::Device::Controller
Version | string | 2.31.1

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Description | string |
Description | string | The Description property provides a textual description of the object.
MappingStrings | string | MIF.DMTF|Video|004.18
Override | string | Description
MaxMemorySupported | uint32 |
Description | string | Maximum amount of memory supported in bytes.
PUnit | string | byte
Units | string | Bytes
NumberOfVideoPages | uint32 |
Description | string | Number of video pages supported given the current resolutions and available memory.
OtherVideoArchitecture | string |
Description | string | A string describing the video architecture type when the instance's VideoArchitecture property is 1 ("Other").
ModelCorrespondence | string | CIM_DisplayController.VideoArchitecture
OtherVideoMemoryType | string |
Description | string | A string describing the video memory type when the instance's VideoMemoryType property is 1 ("Other").
ModelCorrespondence | string | CIM_DisplayController.VideoMemoryType
VideoArchitecture | uint16 |
Description | string | An integer enumeration indicating the display controllers video architecture used to generate the video signal. Usually, a dedicated video processor generates the video signal in accordance with the specified architecture.It is an indicator of the maximum resolution capability of the display controller.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 160, .., 0x8000..
Values | string | Unknown, Other, CGA, EGA, VGA, SVGA, MDA, HGC, MCGA, 8514A, XGA, Linear Frame Buffer, PC-98, DMTF Reserved, Vendor Reserved
VideoMemoryType | uint16 |
Description | string | An integer enumeration indicating the type of video memory.
MappingStrings | string | MIF.DMTF|Video|004.6
ModelCorrespondence | string | CIM_DisplayController.OtherVideoMemoryType
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12
Values | string | Unknown, Other, VRAM, DRAM, SRAM, WRAM, EDO RAM, Burst Synchronous DRAM, Pipelined Burst SRAM, CDRAM, 3DRAM, SDRAM, SGRAM
VideoProcessor | string |
Description | string | A free-form string describing the video processor/Controller.
AcceleratorCapabilities | uint16[] |
ArrayType | string | Indexed
Description | string | An array of integers indicating the graphics and 3D capabilities of the DisplayController.
ModelCorrespondence | string | CIM_DisplayController.CapabilityDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8
Values | string | Unknown, Other, Graphics Accelerator, 3D Accelerator, PCI Fast Write, MultiMonitor Support, PCI Mastering, Second Monochrome Adapter Support, Large Memory Address Support
CapabilityDescriptions | string[] |
ArrayType | string | Indexed
Description | string | An array of free-form strings providing more detailed explanations for any of the video Accelerator features indicated in the Capabilities array. Note, each entry of this array is related to the entry in the Capabilities array that is located at the same index.
ModelCorrespondence | string | CIM_DisplayController.AcceleratorCapabilities

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AllocationState | string | CIM_LogicalDevice
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxNumberControlled | uint32 | CIM_Controller
MaxQuiesceTime | uint64 | CIM_LogicalDevice
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
ProtocolDescription | string | CIM_Controller
ProtocolSupported | uint16 | CIM_Controller
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastReset | datetime | CIM_Controller
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice