# Class CIM_FlatPanel
extends CIM_Display

Capabilities and management of the FlatPanel LogicalDevice.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_UserDevice
|
+--CIM_Display
|
+--CIM_FlatPanel

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of the FlatPanel LogicalDevice.
UMLPackagePath | string | CIM::Device::UserDevices
Version | string | 2.23.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
BuiltIn | uint16 |
Description | string | Defines whether the video output device is built in. 'True' indicates that flat panel is directly attached to a portable computer and 'false' means that flat panel is externally connected through graphics cable (such as VGA) to a computer.
Experimental | boolean | true
ValueMap | string | 0, 2, 3, .., 32768..65535
Values | string | Unknown, True, False, DMTF Reserved, Vendor Reserved
DisplayType | uint16 |
Description | string | An integer enumeration describing the type of flat panel display.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8
Values | string | Unknown, Other, Passive Matrix LCD, Active Matrix LCD, Cholesteric LCD, Field Emission Display, Electro Luminescent Display, Gas Plasma, LED
HorizontalResolution | uint32 |
Description | string | FlatPanel's horizontal resolution in Pixels.
PUnit | string | pixel
Units | string | Pixels
LightSource | uint16 |
Description | string | A description of the display illumination type. For example, backlit (value=2) or reflective (4) can be specified.
ValueMap | string | 0, 1, 2, 3, 4
Values | string | Unknown, Other, Backlit, Edgelit, Reflective
ScanMode | uint16 |
Description | string | A FlatPanel's scan mode indicating either single (value=2) or dual scan (3).
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, Other, Single Scan, Dual Scan
SupportsColor | boolean |
Description | string | Boolean indicating whether the FlatPanel supports color display.
VerticalResolution | uint32 |
Description | string | FlatPanel's vertical resolution in Pixels.
PUnit | string | pixel
Units | string | Pixels

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AllocationState | string | CIM_LogicalDevice
Availability | uint16 | CIM_LogicalDevice
Brightness | uint32 | CIM_Display
Caption | string | CIM_ManagedElement
ColorModePreset | uint16 | CIM_Display
CommunicationStatus | uint16 | CIM_ManagedSystemElement
Contrast | uint32 | CIM_Display
CreationClassName | string | CIM_LogicalDevice
CurrentResolutionH | uint16 | CIM_Display
CurrentResolutionV | uint16 | CIM_Display
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
DisplayMode | uint16 | CIM_Display
DisplayTechnologyType | uint16 | CIM_Display
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
FrequencyH | uint32 | CIM_Display
FrequencyV | uint32 | CIM_Display
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InputSource | uint16 | CIM_Display
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
IsLocked | boolean | CIM_UserDevice
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxBrightness | uint32 | CIM_Display
MaxContrast | uint32 | CIM_Display
MaxQuiesceTime | uint64 | CIM_LogicalDevice
MCCSVersionNumber | string | CIM_Display
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherScalerManufacturerDescription | string | CIM_Display
PerformAutoSetup | uint16 | CIM_Display
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
ScalerManufacturer | uint16 | CIM_Display
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
ColorModePresetCapabilities | uint16[] | CIM_Display
DisplayCharacteristics | uint16[] | CIM_Display
DisplayModeCapabilities | uint16[] | CIM_Display
IdentifyingDescriptions | string[] | CIM_LogicalDevice
InputSourceCapabilities | uint16[] | CIM_Display
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ButtonLock | uint32 | CIM_Display
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreFactoryDefault | uint32 | CIM_Display
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice