# Class CIM_MemoryDiagnosticTest
extends CIM_DiagnosticTest

This class specializes CIM_DiagnosticTest to define the tests specific to system memory.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_DiagnosticService
|
+--CIM_DiagnosticTest
|
+--CIM_MemoryDiagnosticTest

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class specializes CIM_DiagnosticTest to define the tests specific to system memory.
Experimental | boolean | true
UMLPackagePath | string | CIM::System::Diagnostics
Version | string | 2.44.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
MemoryTestType | uint16 |
Description | string | The descriptions for each memory test type are below: * If "Other" (value=1) is set, this test is a vendor extension that performs a custom diagnostic. See ElementName for the name assigned to the test by the vendor. * If "Electrical Wiring" (value=2) is set, this test checks for the existence of a physical memory device, a memory chip, in the system. * If "Data Bus Walking 1s" (value=3) is set, this test verifies the data path from host to target is working properly. * If "Address Bus Walking 1s" (value=4) is set, this test verifies the address path from host to target is working properly. * If "Power-of-Two Addressing" (value=5) is set, this test verifies that the address path from host to target is working properly. That there are no overlapping addresses. * If "Self Addressing" (value=6) is set, this test verifies that the address path from host to target is working properly. *If "Increment and Decrement" (value=7) is set, this test verifies that both the address and data paths from the host to target are working properly. *If "Moving Inversions 0s and 1s" (value=8) is set, this test verifies that both the address and data paths from the host to target are working properly. *If "Moving Inversions Random" (value=9) is set, this test verifies that both the address and data paths from the host to target are working properly. *If "Bit Fade" (value=10) is set, this test verifies that the device is working properly. *If "Reset" (value=11) is set, this test causes a physical memory device, as identified by a logical memory address, to reinitialize itself. *If "Self-Test" (value=12) is set, this test causes the internal components of a physical memory device, as identified by a logical memory address, to be tested. *If "Status" (value=13) is set, this test checks the status of a physical memory device, as identified by a logical memory address. *If "Beacon" (value=14) is set, this test causes at least one of the LEDs of a physical component, as identified by a logical memory address, to flash on and off.
ModelCorrespondence | string | CIM_MemoryDiagnosticTest.OtherMemoryTestTypeDescription
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, .., 0x8000..
Values | string | Unknown, Other, Electrical Wiring, Data Bus Walking 1s, Address Bus Walking 1s, Power-of-Two Addressing, Self Addressing, Increment and Decrement, Moving Inversions 0s and 1s, Moving Inversions Random, Bit Fade, Reset, Self-Test, Status, Beacon, DMTF Reserved, Vendor Reserved
OtherMemoryTestTypeDescription | string |
Description | string | Provides additional information for the MemoryTestType when its value is set to 1 ("Other").
ModelCorrespondence | string | CIM_MemoryDiagnosticTest.MemoryTestType

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
IsInUse | boolean | CIM_DiagnosticTest
LoSID | string | CIM_Service
LoSOrgID | string | CIM_Service
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherCharacteristicDescription | string | CIM_DiagnosticTest
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
Characteristics | uint16[] | CIM_DiagnosticTest
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherCharacteristicsDescriptions | string[] | CIM_DiagnosticTest
OtherTestTypesDescriptions | string[] | CIM_DiagnosticTest
ResourcesUsed | uint16[] | CIM_DiagnosticTest
StatusDescriptions | string[] | CIM_ManagedSystemElement
TestTypes | uint16[] | CIM_DiagnosticTest

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
ClearResults | uint32 | CIM_DiagnosticTest
DiscontinueTest | uint32 | CIM_DiagnosticTest
RequestStateChange | uint32 | CIM_EnabledLogicalElement
RunDiagnostic | uint32 | CIM_DiagnosticService
RunDiagnosticService | uint32 | CIM_DiagnosticService
RunTest | uint32 | CIM_DiagnosticTest
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service