# Class CIM_DiagnosticServiceCapabilities
extends CIM_Capabilities

DiagnosticServiceCapabilities is a class that describes the capabilities of the diagnostic service. This provides the means for the diagnostic service to describe its abilities, limitations, and/or potential for use of various diagnostic service parameters. For example, what types of settings the diagnostic service supports.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_Capabilities
|
+--CIM_DiagnosticServiceCapabilities

## Direct Known Subclasses

CIM_CPUDiagnosticServiceCapabilities
CIM_DiskDriveDiagnosticServiceCapabilities
CIM_EthernetNICDiagnosticServiceCapabilities
CIM_FCHBADiagnosticServiceCapabilities
CIM_MemoryDiagnosticServiceCapabilities
CIM_OpticalDriveDiagnosticServiceCapabilities
CIM_RAIDDiagnosticServiceCapabilities
CIM_StoragePoolDiagnosticServiceCapabilities

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | DiagnosticServiceCapabilities is a class that describes the capabilities of the diagnostic service. This provides the means for the diagnostic service to describe its abilities, limitations, and/or potential for use of various diagnostic service parameters. For example, what types of settings the diagnostic service supports.
UMLPackagePath | string | CIM::System::Diagnostics
Version | string | 2.13.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
SupportedTestWarnings | uint16 | 3
Deprecated | string | CIM_DiagnosticServiceCapabilities.SupportedLogOptions
Description | string | This property is being deprecated because the TestWarningLevel and LogOptions properties serve the same purpose. Lists the level of warning messages that MAY be logged. If for example no warning information is required, the level would be set to "No Warnings" (value=0). Using "Missing Resources" (value=1) will cause warnings to be generated when required resources or hardware are not found. Setting the value to 2, "Testing Impacts", results in both missing resources and 'test impact' warnings (for example, multiple retries required) to be reported.
ValueMap | string | 2, 3, 4, 5
Values | string | No Warnings, Missing Resources, Testing Impacts, All Warnings
OtherSupportedExecutionControlsDescriptions | string[] |
ArrayType | string | Indexed
Description | string | Provides additional information for SupportedExecutionControls when the corresponding value is set ("Other").
ModelCorrespondence | string | CIM_DiagnosticServiceCapabilities.SupportedExecutionControls
OtherSupportedLogOptionsDescriptions | string[] |
ArrayType | string | Indexed
Description | string | Provides additional information for SupportedLogOptions when the corresponding value is set to 1 ("Other").
ModelCorrespondence | string | CIM_DiagnosticServiceCapabilities.SupportedLogOptions
OtherSupportedLogStorageDescriptions | string[] |
ArrayType | string | Indexed
Description | string | Provides additional information for SupportedLogStorage when the corresponding value is set to 1 ("Other").
ModelCorrespondence | string | CIM_DiagnosticServiceCapabilities.SupportedLogStorage
OtherSupportedLoopControlDescriptions | string[] |
ArrayType | string | Indexed
Description | string | Provides additional information for SupportedLoopControl when the corresponding value is set to 1 ("Other").
ModelCorrespondence | string | CIM_DiagnosticServiceCapabilities.SupportedLoopControl
OtherSupportedServiceModesDescriptions | string[] |
ArrayType | string | Indexed
Description | string | Provides additional information for SupportedServiceModes when the corresponding value is set to 1 ("Other").
ModelCorrespondence | string | CIM_DiagnosticServiceCapabilities.SupportedServiceModes
SupportedExecutionControls | uint16[] |
Description | string | The SupportedExecutionControls property lists the job controls that are supported by the Diagnostic Service. The values are: (Value = 2) is deprecated. Previous versions defined this as "Job Creation" and was intended to indicate that a ConcreteJob instance will be created to control the diagnostic job launched by the diagnostic service. Since Job creation is REQUIRED, this attribute value is unnecessary and confusing. "Kill Job" (Value = 3): publishes that the diagnostic service implements the ConcreteJob.RequestStateChange(Kill) method. "Suspend Job" (Value = 4): publishes that the diagnostic service implements the ConcreteJob.RequestStateChange(Suspend) method. "Terminate Job" (Value = 5): publishes that the diagnostic service implements the ConcreteJob.RequestStateChange(Terminate) method.
ModelCorrespondence | string | CIM_DiagnosticServiceCapabilities.OtherSupportedExecutionControlsDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5, 0x8000
Values | string | Unknown, Other, Reserved, Kill Job, Suspend Job, Terminate Job, No Execution Controls
SupportedLogOptions | uint16[] |
ArrayType | string | Indexed
Description | string | The SupportedLogOptions property lists the log options that are supported by the Diagnostic Service.
ModelCorrespondence | string | CIM_DiagnosticSettingData.LogOptions, CIM_DiagnosticServiceCapabilities.OtherSupportedLogOptionsDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 0x8000
Values | string | Unknown, Other, Results, Subtests, Actions, Warnings, Status, Device Errors, Service Errors, Setting Data, Statistics, Hardware Configuration, Software Configuration, References, Debug, No Log Options
SupportedLogStorage | uint16[] |
Description | string | The SupportedLogStorage property lists the storage options for logging that are supported by the Diagnostic Service. The values are: "DiagnosticLog" (Value = 2): Supports use of the DiagnosticLog class for aggregating DiagnosticRecords. "MessageLog" (Value = 3): Supports writing log information using the methods in the MessageLog class. "File" (Value = 4): Supports writing log information to a file.
ModelCorrespondence | string | CIM_DiagnosticServiceCapabilities.OtherSupportedLogStorageDescriptions, CIM_DiagnosticSettingData.LogStorage
ValueMap | string | 0, 1, 2, 3, 4, 0x8000
Values | string | Unknown, Other, DiagnosticLog, MessageLog, File, No Log Storage
SupportedLoopControl | uint16[] |
ArrayType | string | Indexed
Description | string | The SupportedLoopControl property lists the loop controls that are supported by the Diagnostic Service.
ModelCorrespondence | string | CIM_DiagnosticSettingData.LoopControl, CIM_DiagnosticServiceCapabilities.OtherSupportedLoopControlDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5, 0x8000
Values | string | Unknown, Other, Continuous, Count, Timer, ErrorCount, No Loop Control
SupportedServiceModes | uint16[] |
ArrayType | string | Indexed
Description | string | The SupportedServiceModes property lists the operational modes that are supported by the Diagnostic Service. These modes may correspond to, but are not limited to, settings that may be applied to a Diagnostic Service.
ModelCorrespondence | string | CIM_DiagnosticServiceCapabilities.OtherSupportedServiceModesDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 0x8000
Values | string | Unknown, Other, PercentOfTestCoverage, QuickMode, HaltOnError, ResultPersistence, QueryTimeout, NonDestructive, No Service Modes

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_Capabilities
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_Capabilities

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
CreateGoalSettings | uint16 | CIM_Capabilities