# Class CIM_PlatformWatchdogService
extends CIM_Service

PlatformWatchdogService is class derived from Service that provides the controls to manage the watchdog timer service of a managed element. A PlatformWatchdogService monitors the ability of a monitored entity to reset a countdown timer before it expires. If the timer expires, the service may take specific action upon expiration. The monitored entity may be the Operating System, BIOS, or a software component that is installed on the computer system.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_PlatformWatchdogService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | PlatformWatchdogService is class derived from Service that provides the controls to manage the watchdog timer service of a managed element. A PlatformWatchdogService monitors the ability of a monitored entity to reset a countdown timer before it expires. If the timer expires, the service may take specific action upon expiration. The monitored entity may be the Operating System, BIOS, or a software component that is installed on the computer system.
UMLPackagePath | string | CIM::System::Watchdog
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ActionOnExpiration | uint16 |
Description | string | ActionOnExpiration specifies the action that should happen upon the expiration of the watchdog timer. A value set to 1 = "Other" shall indicate that the action described in OtherActionOnExpiration is to be taken. A value set to 2 = "None - Status Only" shall indicate that no action is to be taken. A value set to 3 = "System Reset" shall indicate that the action is to reset the system. A value set to 4 = "System Power Off" shall indicate that the action is to power off the system. A value set to 5 = "System Power Off, then On" shall indicate that the action is to power off the system, followed by a power-on of the system. A value set to 6 = "Generate System NonMaskableInterrupt (NMI)" shall indicate that the action is to generate a non-maskable interrupt on the system. A value set to 7 = "Generate System Management Interrupt (SMI)" shall indicate that the action is to generate a management interrupt on the system. A value set to 8 = " Reset Monitored Entity " shall indicate that the action is to reset the monitored entity.
ModelCorrespondence | string | CIM_PlatformWatchdogService.OtherActionOnExpiration
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8
Values | string | Unknown, Other, None - Status Only, System Reset, System Power Off, System Power Off, then On, Generate System NonMaskableInterrupt (NMI), Generate System Management Interrupt (SMI), Reset Monitored Entity
CurrentTimerValue | datetime |
Description | string | The amount of time remaining before the watchdog timer expires. A value of NULL shall mean unknown.
MonitoredEntityType | uint16 |
Description | string | The type of entity that is monitored by the PlatformWatchdogService. This property is used to identify the type of entity that is responsible for re-arming, or whose information is used to re-arm, the watchdog at periodic intervals. A value set to 2 = "Operating System" shall indicate that the entity is an operating system. A value set to 3 = "Operating System Boot Process" shall indicate that the entity is one which handles the process of booting an operating system. A value set to 4 = "Operating System Shutdown Process" shall indicate that the entity is one which handles process of shutting down of an operating system. A value set to 5 = "Firmware Boot Process" shall indicate that the entity is one which handles process of booting firmware. A value set to 6 = "BIOS Boot Process" shall indicate that the entity is one which handles process of booting the system BIOS. A value set to 7 = "Application" shall indicate that the entity is an application. A value set to 8 = "Service Processor" shall indicate that the entity is an service processor.
ModelCorrespondence | string | CIM_PlatformWatchdogService.OtherMonitoredEntityTypeDescription
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8
Values | string | Unknown, Other, Operating System, Operating System Boot Process, Operating System Shutdown Process, Firmware Boot Process, BIOS Boot Process, Application, Service Processor
OtherActionOnExpiration | string |
Description | string | This property shall have a value if ActionOnExpiration contains the value 1 (Other).
ModelCorrespondence | string | CIM_PlatformWatchdogService.ActionOnExpiration
OtherMonitoredEntityTypeDescription | string |
Description | string | A string that describes the type of monitored entity when MonitoredEntityType is set to 1 (Other).
MaxLen | uint32 | 256
ModelCorrespondence | string | CIM_PlatformWatchdogService.MonitoredEntityType
TimeOfLastExpiration | datetime |
Description | string | The time of the last watchdog timer expiration.
TimeoutInterval | datetime |
Description | string | The timeout interval that is used by the watchdog.
TimerExpired | boolean |
Description | string | TimerExpired indicates when the watchdog timer has expired. A value of False shall indicate the watchdog timer did not expire the last time it was active, or this information is unknown. A value of True shall indicate the watchdog timer expired the last time it was active. If CurrentTimerValue is supported it also expresses this same information when it has the value 00000000000000.000000:000 expressed in the interval notation of the datetime type.
TimerResolution | datetime |
Description | string | The resolution of the timer used by the watchdog. The timer can expire anytime between (TimeoutInterval - TimerResolution) or (TimeoutInterval + TimerResolution).

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LoSID | string | CIM_Service
LoSOrgID | string | CIM_Service
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
RequestStateChange | uint32 | CIM_EnabledLogicalElement
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service