# Class CIM_VLANEndpoint
extends CIM_ProtocolEndpoint

An endpoint on a switch or endstation which is assigned to a given VLAN or accepts traffic from one or more VLANs. As defined by the property, OperationalEndpointMode, the endpoint may be configured as trunking or nontrunking. Note that an endpoint may dynamically be converted to/from a trunking mode. When this occurs, simply update the OperationalEndpointMode property. This class is associated with a DataLink or IPProtocol Endpoint - as another aspect of that endpoint - using the LogicalIdentity relationship. In this case, the VLANEndpoint takes the role of SameElement.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_ProtocolEndpoint
|
+--CIM_VLANEndpoint

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | An endpoint on a switch or endstation which is assigned to a given VLAN or accepts traffic from one or more VLANs. As defined by the property, OperationalEndpointMode, the endpoint may be configured as trunking or nontrunking. Note that an endpoint may dynamically be converted to/from a trunking mode. When this occurs, simply update the OperationalEndpointMode property. This class is associated with a DataLink or IPProtocol Endpoint - as another aspect of that endpoint - using the LogicalIdentity relationship. In this case, the VLANEndpoint takes the role of SameElement.
UMLPackagePath | string | CIM::Network::VLAN
Version | string | 2.26.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
DesiredEndpointMode | uint16 |
Description | string | The desired VLAN mode that is requested for use. (Note that the current mode is given by the OperationalEndpointMode property.) The following values are defined: - Access: Puts the endpoint/switch port into permanent nontrunking mode and negotiates to convert the link into a nontrunk link. The endpoint becomes a nontrunk interface. - Dynamic Auto: Makes the endpoint able to convert the link to a trunk link. The endpoint becomes a trunk interface if the neighboring interface is set to trunk or desirable mode. - Dynamic Desirable: Makes the endpoint actively attempt to convert the link to a trunk link. The endpoint becomes a trunk interface if the neighboring interface is set to trunk, desirable, or auto mode. The default switch-port mode for all Ethernet interfaces is 'dynamic desirable.' - Trunk: Puts the endpoint into permanent trunking mode and negotiates to convert the link into a trunk link. The endpoint becomes a trunk interface even if the neighboring interface is not a trunk interface. - Dot1Q Tunnel: Configures the interface as a tunnel (nontrunking) endpoint/port to be connected in an asymmetric link with an 802.1Q trunk port. 802.1Q tunneling is used to maintain customer VLAN integrity across a service provider network.
ModelCorrespondence | string | CIM_VLANEndpoint.OperationalEndpointMode, CIM_VLANEndpoint.OtherEndpointMode
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7..32767, ..
Values | string | DMTF Reserved, Other, Access, Dynamic Auto, Dynamic Desirable, Trunk, Dot1Q Tunnel, DMTF Reserved, Vendor Reserved
Write | boolean | true
DesiredVLANTrunkEncapsulation | uint16 |
Description | string | The type of VLAN encapsulation that is requested for use. (Note that the encapsulation currently in use is given by the OperationalVLANTrunkEncapsulation property.) Note that this property is only applicable when the endpoint is operating in a trunking mode (see the OperationalEndpointMode property for additional details). This property is either 'not applicable' (i.e., the endpoint will never be placed in a trunking mode), a particular type (802.1q or Cisco ISL), or 'negotiate' (i.e., the result of the negotiation between this interface and its neighbor). The value, 'Negotiate' is not allowed if the endpoint does not support negotiation. This capability is hardware and vendor dependent. Refer to the associated VLANEndpointCapabilities.doesTrunkEncapsulationNegotiation property to validate whether a particular endpoint (port) supports encapsulation negotiation.
ModelCorrespondence | string | CIM_VLANEndpoint.OperationalVLANTrunkEncapsulation, CIM_VLANEndpoint.OtherTrunkEncapsulation
ValueMap | string | 0, 1, 2, 3, 4, 5, 6..32767, 32768..
Values | string | DMTF Reserved, Other, Not Applicable, 802.1q, Cisco ISL, Negotiate, DMTF Reserved, Vendor Reserved
Write | boolean | true
GVRPStatus | uint16 |
Description | string | Indicates whether GARP VLAN Registration Protocol (GVRP) is enabled or disabled on the trunk endpoint/port. This property is 'not applicable' unless GVRP is supported by the endpoint. This is indicated in the Capabilities property, VLANEndpointCapabilities.Dot1QTagging. This property is applicable only when the endpoint is operating in trunking mode (determined by examining the SwitchEndpointMode property).
ModelCorrespondence | string | CIM_VLANEndpoint.OperationalEndpointMode, CIM_VLANEndpointCapabilities.Dot1QTagging
ValueMap | string | 0, 2, 3, 4
Values | string | Unknown, Not Applicable, Enabled, Disabled
OperationalEndpointMode | uint16 |
Description | string | The configuration mode for the VLAN endpoint. The following values are defined: /n - Unknown: If the endpoint is not VLAN aware. /n - Access: Puts the endpoint into permanent nontrunking mode and negotiates to convert the link into a nontrunk link. The endpoint becomes a nontrunk interface. - Dynamic Auto: Makes the endpoint able to convert the link to a trunk link. The endpoint becomes a trunk interface if the neighboring interface is set to trunk or desirable mode. - Dynamic Desirable: Makes the endpoint actively attempt to convert the link to a trunk link. The endpoint becomes a trunk interface if the neighboring interface is set to trunk, desirable, or auto mode. The default switch-port mode for all Ethernet interfaces is 'dynamic desirable.' - Trunk: Puts the endpoint into permanent trunking mode and negotiates to convert the link into a trunk link. The endpoint becomes a trunk interface even if the neighboring interface is not a trunk interface. - Dot1Q Tunnel: Configures the interface as a tunnel (nontrunking) endpoint/port to be connected in an asymmetric link with an 802.1Q trunk port. 802.1Q tunneling is used to maintain customer VLAN integrity across a service provider network.
ModelCorrespondence | string | CIM_VLANEndpoint.DesiredEndpointMode, CIM_VLANEndpoint.OtherEndpointMode
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7..32767, ..
Values | string | DMTF Reserved, Other, Access, Dynamic Auto, Dynamic Desirable, Trunk, Dot1Q Tunnel, DMTF Reserved, Vendor Reserved
OperationalVLANTrunkEncapsulation | uint16 |
Description | string | The type of VLAN encapsulation in use on a trunk endpoint/port. This property is either 'not applicable' (i.e., the endpoint is not operating in trunking mode), a particular type (802.1q or Cisco ISL), 'negotiating' (i.e., the endpoints are negotiating the encapsulation type). Note that this property is only applicable when the endpoint is operating in a trunking mode (see the OperationalEndpointMode property for additional details).
ModelCorrespondence | string | CIM_VLANEndpoint.OtherTrunkEncapsulation, CIM_VLANEndpoint.DesiredVLANTrunkEncapsulation
ValueMap | string | 0, 1, 2, 3, 4, 5, 6..32767, 32768..
Values | string | Unknown, Other, Not Applicable, 802.1q, Cisco ISL, Negotiating, DMTF Reserved, Vendor Reserved
OtherEndpointMode | string |
Description | string | A string describing the type of VLAN endpoint model that is supported by this VLANEndpoint, when the value of the mode property is set to 1 (i.e., "Other"). This property should be set to NULL when the mode property is any value other than 1.
ModelCorrespondence | string | CIM_VLANEndpoint.DesiredEndpointMode, CIM_VLANEndpoint.OperationalEndpointMode
Write | boolean | true
OtherTrunkEncapsulation | string |
Description | string | A string describing the type of VLAN encapsulation that is supported by this VLANEndpoint, when the value of the encapsulation property is set to 1 (i.e., "Other"). This property should be set to NULL when the desired encapsulation property is any value other than 1.
ModelCorrespondence | string | CIM_VLANEndpoint.DesiredVLANTrunkEncapsulation, CIM_VLANEndpoint.OperationalVLANTrunkEncapsulation
Write | boolean | true

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
BroadcastResetSupported | boolean | CIM_ProtocolEndpoint
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_ServiceAccessPoint
Description | string | CIM_ProtocolEndpoint
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_ProtocolEndpoint
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
Name | string | CIM_ProtocolEndpoint
NameFormat | string | CIM_ProtocolEndpoint
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherTypeDescription | string | CIM_ProtocolEndpoint
PrimaryStatus | uint16 | CIM_ManagedSystemElement
ProtocolIFType | uint16 | CIM_ProtocolEndpoint
ProtocolType | uint16 | CIM_ProtocolEndpoint
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_ServiceAccessPoint
SystemName | string | CIM_ServiceAccessPoint
TimeOfLastStateChange | datetime | CIM_ProtocolEndpoint
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ProtocolEndpoint
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
BroadcastReset | uint32 | CIM_ProtocolEndpoint
RequestStateChange | uint32 | CIM_EnabledLogicalElement