# Class CIM_VoltageSensor
extends CIM_NumericSensor

The use of this class is being deprecated in lieu of the additions to Sensor and NumericSensor. A VoltageSensor can be defined by setting the SensorType property, inherited from Sensor, to 3 ("Voltage").

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Sensor
|
+--CIM_NumericSensor
|
+--CIM_VoltageSensor

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_NumericSensor
Description | string | The use of this class is being deprecated in lieu of the additions to Sensor and NumericSensor. A VoltageSensor can be defined by setting the SensorType property, inherited from Sensor, to 3 ("Voltage").
UMLPackagePath | string | CIM::Device::Sensors
Version | string | 2.8.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Accuracy | sint32 |
Deprecated | string | No value
Description | string | Indicates the accuracy of the Sensor for the measured property. Its value is recorded as plus/minus hundredths of a percent. Accuracy, along with Resolution, is used to calculate the actual value of the measured physical property. Accuracy may vary depending on whether the Device is linear over its dynamic range.
MappingStrings | string | MIF.DMTF|Voltage Probe|001.19
Override | string | Accuracy
PUnit | string | percent * 10^-2
Units | string | Hundredths of Percent
BaseUnits | uint16 | 5
Deprecated | string | No value
Description | string | The base unit of the values returned by this Sensor. All the values returned by this Sensor are represented in the units obtained by (BaseUnits * 10 raised to the power of the UnitModifier). For example, if BaseUnits is Volts and the UnitModifier is -6, then the units of the values returned are MicroVolts. However, if the RateUnits property is set to a value other than "None", then the units are further qualified as rate units. In the above example, if RateUnits is set to "Per Second", then the values returned by the Sensor are in MicroVolts/Second. The units apply to all numeric properties of the Sensor, unless explicitly overridden by the Units qualifier.
ModelCorrespondence | string | CIM_NumericSensor.UnitModifier, CIM_NumericSensor.RateUnits
Override | string | BaseUnits
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, 62, 63, 64, 65, 66
Values | string | Unknown, Other, Degrees C, Degrees F, Degrees K, Volts, Amps, Watts, Joules, Coulombs, VA, Nits, Lumens, Lux, Candelas, kPa, PSI, Newtons, CFM, RPM, Hertz, Seconds, Minutes, Hours, Days, Weeks, Mils, Inches, Feet, Cubic Inches, Cubic Feet, Meters, Cubic Centimeters, Cubic Meters, Liters, Fluid Ounces, Radians, Steradians, Revolutions, Cycles, Gravities, Ounces, Pounds, Foot-Pounds, Ounce-Inches, Gauss, Gilberts, Henries, Farads, Ohms, Siemens, Moles, Becquerels, PPM (parts/million), Decibels, DbA, DbC, Grays, Sieverts, Color Temperature Degrees K, Bits, Bytes, Words (data), DoubleWords, QuadWords, Percentage, Pascals
CurrentReading | sint32 |
Deprecated | string | No value
Description | string | The current value indicated by the Sensor.
MappingStrings | string | MIF.DMTF|Voltage Probe|001.5
Override | string | CurrentReading
LowerThresholdCritical | sint32 |
Deprecated | string | No value
Description | string | The Sensor's threshold values specify the ranges (min and max values) for determining whether the Sensor is operating under Normal, NonCritical, Critical or Fatal conditions. If the CurrentReading is between LowerThresholdCritical and Lower ThresholdFatal, then the CurrentState is Critical.
MappingStrings | string | MIF.DMTF|Voltage Probe|001.13
Override | string | LowerThresholdCritical
Write | boolean | true
LowerThresholdFatal | sint32 |
Deprecated | string | No value
Description | string | The Sensor's threshold values specify the ranges (min and max values) for determining whether the Sensor is operating under Normal, NonCritical, Critical or Fatal conditions. If the CurrentReading is below LowerThresholdFatal, then the Current State is Fatal.
MappingStrings | string | MIF.DMTF|Voltage Probe|001.15
Override | string | LowerThresholdFatal
Write | boolean | true
LowerThresholdNonCritical | sint32 |
Deprecated | string | No value
Description | string | The Sensor's threshold values specify the ranges (min and max values) for determining whether the Sensor is operating under Normal, NonCritical, Critical or Fatal conditions. If Current Reading is between LowerThresholdNonCritical and Upper ThresholdNonCritical, then the Sensor is reporting a normal value. If CurrentReading is between LowerThresholdNonCritical and LowerThresholdCritical, then the CurrentState is NonCritical.
MappingStrings | string | MIF.DMTF|Voltage Probe|001.11
Override | string | LowerThresholdNonCritical
Write | boolean | true
MaxReadable | sint32 |
Deprecated | string | No value
Description | string | MaxReadable indicates the largest value of the measured property that can be read by the NumericSensor.
MappingStrings | string | MIF.DMTF|Voltage Probe|001.9
Override | string | MaxReadable
MinReadable | sint32 |
Deprecated | string | No value
Description | string | MinReadable indicates the smallest value of the measured property that can be read by the NumericSensor.
MappingStrings | string | MIF.DMTF|Voltage Probe|001.10
Override | string | MinReadable
NominalReading | sint32 |
Deprecated | string | No value
Description | string | NominalReading indicates the 'normal' or expected value for the NumericSensor.
MappingStrings | string | MIF.DMTF|Voltage Probe|001.6
Override | string | NominalReading
NormalMax | sint32 |
Deprecated | string | No value
Description | string | NormalMax provides guidance for the user as to the normal maximum range for the NumericSensor.
MappingStrings | string | MIF.DMTF|Voltage Probe|001.7
Override | string | NormalMax
NormalMin | sint32 |
Deprecated | string | No value
Description | string | NormalMin provides guidance for the user as to the normal minimum range for the NumericSensor.
MappingStrings | string | MIF.DMTF|Voltage Probe|001.8
Override | string | NormalMin
RateUnits | uint16 | 0
Deprecated | string | No value
Description | string | Specifies if the units returned by this Sensor are rate units. All the values returned by this Sensor are represented in the units obtained by (BaseUnits * 10 raised to the power of the UnitModifier). This is true unless this property (RateUnits) has a value different than "None". For example, if BaseUnits is Volts and the UnitModifier is -6, then the units of the values returned are MicroVolts. But, if the RateUnits property is set to a value other than "None", then the units are further qualified as rate units. In the above example, if RateUnits is set to "Per Second", then the values returned by the Sensor are in MicroVolts/Second. The units apply to all numeric properties of the Sensor, unless explicitly overridden by the Units qualifier. Any implementation of CurrentReading should be qualified with either a Counter or a Gauge qualifier, depending on the characteristics of the sensor being modeled.
ModelCorrespondence | string | CIM_NumericSensor.UnitModifier, CIM_NumericSensor.BaseUnits
Override | string | RateUnits
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9
Values | string | None, Per MicroSecond, Per MilliSecond, Per Second, Per Minute, Per Hour, Per Day, Per Week, Per Month, Per Year
Resolution | uint32 |
Deprecated | string | No value
Description | string | Resolution indicates the ability of the Sensor to resolve differences in the measured property. The units for this measurement are determined by BaseUnit*UnitModifier/RateUnit.
MappingStrings | string | MIF.DMTF|Voltage Probe|001.17
Override | string | Resolution
PUnit | string | volt * 10^-4
Units | string | Tenths of MilliVolts
SensorType | uint16 | 3
Deprecated | string | No value
Description | string | The Type of the Sensor, e.g. Voltage or Temperature Sensor. If the type is set to "Other", then the OtherSensorType Description can be used to further identify the type, or if the Sensor has numeric readings, then the type of the Sensor can be implicitly determined by the Units. A description of the different Sensor types is as follows: A Temperature Sensor measures the environmental temperature. Voltage and Current Sensors measure electrical voltage and current readings. A Tachometer measures speed/revolutions of a Device. For example, a Fan Device can have an associated Tachometer which measures its speed. A Counter is a general purpose Sensor that measures some numerical property of a Device. A Counter value can be cleared, but it never decreases. A Switch Sensor has states like Open/Close, On/Off, or Up/Down. A Lock has states of Locked/Unlocked. Humidity, Smoke Detection and Air Flow Sensors measure the equivalent environmental characteristics. A Presence Sensor detects the presence of a PhysicalElement. A Power Consumption Sensor measures the instantaneous power consumed by a managed element. A Power Production Sensor measures the instantaneous power produced by a managed element such as a power supply or a voltage regulator. A pressure sensor is used to report pressure. Intrusion sensor reports an intrusion of an enclosure regardless whether it was authorized or not.
ModelCorrespondence | string | CIM_Sensor.OtherSensorTypeDescription
Override | string | SensorType
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, .., 32768..65535
Values | string | Unknown, Other, Temperature, Voltage, Current, Tachometer, Counter, Switch, Lock, Humidity, Smoke Detection, Presence, Air Flow, Power Consumption, Power Production, Pressure, Intrusion, DMTF Reserved, Vendor Reserved
Tolerance | sint32 |
Deprecated | string | No value
Description | string | This property is being deprecated in lieu of using the Resolution and Accuracy properties. Indicates the tolerance of the Sensor for the measured property. Tolerance, along with Resolution and Accuracy, is used to calculate the actual value of the measured physical property. Tolerance may vary depending on whether the Device is linear over its dynamic range.
MappingStrings | string | MIF.DMTF|Voltage Probe|001.18
Override | string | Tolerance
UnitModifier | sint32 | -3
Deprecated | string | No value
Description | string | The unit multiplier for the values returned by this Sensor. All the values returned by this Sensor are represented in the units obtained by (BaseUnits * 10 raised to the power of the UnitModifier). For example, if BaseUnits is Volts and the Unit Modifier is -6, then the units of the values returned are MicroVolts. However, if the RateUnits property is set to a value other than "None", then the units are further qualified as rate units. In the above example, if RateUnits is set to "Per Second", then the values returned by the Sensor are in MicroVolts/Second. The units apply to all numeric properties of the Sensor, unless explicitly overridden by the Units qualifier.
ModelCorrespondence | string | CIM_NumericSensor.BaseUnits, CIM_NumericSensor.RateUnits
Override | string | UnitModifier
UpperThresholdCritical | sint32 |
Deprecated | string | No value
Description | string | The Sensor's threshold values specify the ranges (min and max values) for determining whether the Sensor is operating under Normal, NonCritical, Critical or Fatal conditions. If the CurrentReading is between UpperThresholdCritical and Upper ThresholdFatal, then the CurrentState is Critical.
MappingStrings | string | MIF.DMTF|Voltage Probe|001.14
Override | string | UpperThresholdCritical
Write | boolean | true
UpperThresholdFatal | sint32 |
Deprecated | string | No value
Description | string | The Sensor's threshold values specify the ranges (min and max values) for determining whether the Sensor is operating under Normal, NonCritical, Critical or Fatal conditions. If the CurrentReading is above UpperThresholdFatal, then the Current State is Fatal.
MappingStrings | string | MIF.DMTF|Voltage Probe|001.16
Override | string | UpperThresholdFatal
Write | boolean | true
UpperThresholdNonCritical | sint32 |
Deprecated | string | No value
Description | string | The Sensor's threshold values specify the ranges (min and max values) for determining whether the Sensor is operating under Normal, NonCritical, Critical or Fatal conditions. If the CurrentReading is between LowerThresholdNonCritical and UpperThresholdNonCritical, then the Sensor is reporting a normal value. If the CurrentReading is between UpperThreshold NonCritical and UpperThresholdCritical, then the CurrentState is NonCritical.
MappingStrings | string | MIF.DMTF|Voltage Probe|001.12
Override | string | UpperThresholdNonCritical
Write | boolean | true

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AllocationState | string | CIM_LogicalDevice
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
CurrentState | string | CIM_Sensor
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
Hysteresis | uint32 | CIM_NumericSensor
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
IsLinear | boolean | CIM_NumericSensor
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherSensorTypeDescription | string | CIM_Sensor
PollingInterval | uint64 | CIM_Sensor
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
SensorContext | string | CIM_Sensor
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
EnabledThresholds | uint16[] | CIM_NumericSensor
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PossibleStates | string[] | CIM_Sensor
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
SettableThresholds | uint16[] | CIM_NumericSensor
StatusDescriptions | string[] | CIM_ManagedSystemElement
SupportedThresholds | uint16[] | CIM_NumericSensor

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
GetNonLinearFactors | uint32 | CIM_NumericSensor
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreDefaultThresholds | uint32 | CIM_NumericSensor
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice