# Class CIM_DiskDrive
extends CIM_MediaAccessDevice

Capabilities and managment of a DiskDrive, a subtype of MediaAccessDevice.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_MediaAccessDevice
|
+--CIM_DiskDrive

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and managment of a DiskDrive, a subtype of MediaAccessDevice.
UMLPackagePath | string | CIM::Device::StorageDevices
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
DiskType | uint16 |
Description | string | The technology used to store data. the hybrid uses a combination of HDD and SSD in the same drive.
ValueMap | string | 0, 1, 2, 3, 4
Values | string | Unknown, Other, Hard Disk Drive, Solid State Drive, Hybrid
Encryption | uint16 |
Description | string | This property reflects the state of the encryption feature implemented by some disk drives as defined by SCSI. The Unlocked state means the drive is capable of encryption but it is disabled. The Locked state means the drive is currently encrypted
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, Not Supported, Unlocked, Locked
FormFactor | uint16 |
Description | string | The Physical size of the disk drive.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6
Values | string | Unknown, Other, Not Reported, 5.25 inch, 3.5 inch, 2.5 inch, 1.8 inch
InterconnectSpeed | uint64 |
Description | string | This property identifies the port speed in bit/second. If the speed is unknown the property should be set to 0.
InterconnectType | uint16 |
Description | string | This property identifies the drive interface type. ATA: Advanced Technology Attachment SATA: Serial ATA SAS: Serial Attached SCSI FC: Fibre Channel SOP: SCSI Over PCIe -- Peripheral Component Interconnect express.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7
Values | string | Unknown, Other, Not Applicable, ATA, SATA, SAS, FC, SOP
OtherInterconnectType | string |
Description | string | This property identifies other interconnect types.
RPM | uint32 |
Description | string | This property identifies how fast the drive media spins in Rotations Per Minute. Solid State drives should set this property to 0. If the RPM is unknown the property should be set to 0xFFFFFFFF
PUnit | string | revolution / minute
Units | string | Revolutions per Minute

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AllocationState | string | CIM_LogicalDevice
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CompressionMethod | string | CIM_MediaAccessDevice
CreationClassName | string | CIM_LogicalDevice
DefaultBlockSize | uint64 | CIM_MediaAccessDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
ErrorMethodology | string | CIM_MediaAccessDevice
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastCleaned | datetime | CIM_MediaAccessDevice
LastErrorCode | uint32 | CIM_LogicalDevice
LoadTime | uint64 | CIM_MediaAccessDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxAccessTime | uint64 | CIM_MediaAccessDevice
MaxBlockSize | uint64 | CIM_MediaAccessDevice
MaxMediaSize | uint64 | CIM_MediaAccessDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
MaxUnitsBeforeCleaning | uint64 | CIM_MediaAccessDevice
MediaIsLocked | boolean | CIM_MediaAccessDevice
MinBlockSize | uint64 | CIM_MediaAccessDevice
MountCount | uint64 | CIM_MediaAccessDevice
Name | string | CIM_ManagedSystemElement
NeedsCleaning | boolean | CIM_MediaAccessDevice
NumberOfMediaSupported | uint32 | CIM_MediaAccessDevice
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Security | uint16 | CIM_MediaAccessDevice
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastMount | datetime | CIM_MediaAccessDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalMountTime | uint64 | CIM_MediaAccessDevice
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
UncompressedDataRate | uint32 | CIM_MediaAccessDevice
UnitsDescription | string | CIM_MediaAccessDevice
UnitsUsed | uint64 | CIM_MediaAccessDevice
UnloadTime | uint64 | CIM_MediaAccessDevice
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
Capabilities | uint16[] | CIM_MediaAccessDevice
CapabilityDescriptions | string[] | CIM_MediaAccessDevice
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
LockMedia | uint32 | CIM_MediaAccessDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice