# Class CIM_CLPSettingData
extends CIM_SettingData

A representation of the SettingData of a CLProtocol. The relationship between the SettingData and the CLP Service is described by instantiating the ProvidesEndpoint association, with an association to the transport (TelnetProtocolEndpoint or SSHProtocolEndpoint) with a BindsTo association.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_CLPSettingData

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | A representation of the SettingData of a CLProtocol. The relationship between the SettingData and the CLP Service is described by instantiating the ProvidesEndpoint association, with an association to the transport (TelnetProtocolEndpoint or SSHProtocolEndpoint) with a BindsTo association.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::ProtocolEndpoints
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CurrentDefaultTarget | string |
Description | string | Identifies the initial Current Default Target when a CLP Session is established. The Current Default Target is the CLP session environment setting that establishes a default base address for all command targets that are expressed as a relative target address and is used as the command target if no command target is specified in a command. The CLP specification requires this value to be fixed at the root of the address space being managed. Therefore this value does not have a write qualifier.
ModelCorrespondence | string | CIM_CLPProtocolEndpoint.CurrentDefaultTarget
DisplayOption | string |
Description | string | Establishes the default value for the display option. The argument string is stored "as-is" without normalization beyond capitalization. The argument string is compliant with the SM CLP command line grammar.
ModelCorrespondence | string | CIM_CLPProtocolEndpoint.DisplayOption
Write | boolean | true
KeepTime | uint16 |
Description | string | Establishes the amount of time in seconds that the CLP Session should retain a CLP command job status. A KeepTime value of zero shall be interpreted to mean keep forever.
ModelCorrespondence | string | CIM_CLPProtocolEndpoint.KeepTime
PUnit | string | second
Units | string | Seconds
Write | boolean | true
OutputCount | uint32 |
Description | string | Establishes the default CLP Session command output count number when multiple items are returned in the output as described in SM CLP Specification, DMTF document DSP0214. The value 0xFFFFFFFF shall be interpreted to mean that all items are to be returned. The maximum value for the count number is determined by the class of the target.
ModelCorrespondence | string | CIM_CLPProtocolEndpoint.OutputCount
Write | boolean | true
OutputFormat | uint16 |
Description | string | OutputFormat establishes the default CLP Session command output format, as described in SM CLP Specification, DMTF document DSP0214.
ModelCorrespondence | string | CIM_CLPProtocolEndpoint.OutputFormat
ValueMap | string | 2, 3, 4, 5, .., 0x8000..0xFFFF
Values | string | Text, clpcsv, Keyword, clpxml, DMTF Reserved, Vendor Reserved
Write | boolean | true
OutputLanguage | string |
Description | string | Establishes the default CLP Session command output language. As described in SM CLP Specification, DMTF document DSP0214, the language value is a 3-character string identifier of language as specified in ISO 639.2; "eng" is the default.
Write | boolean | true
OutputOrder | uint16 |
Description | string | OutputOrder establishes the default CLP Session command output order when multiple items are returned in the command output as described in SM CLP Specification, DMTF document DSP0214.
ModelCorrespondence | string | CIM_CLPProtocolEndpoint.OutputOrder
ValueMap | string | 2, 3, .., 0x8000..0xFFFF
Values | string | Default, Reverse, DMTF Reserved, Vendor Reserved
Write | boolean | true
OutputPosition | uint16 |
Description | string | OutputPosition establishes the default CLP Session command output beginning position when multiple items are returned in the command output, as described in SM CLP Specification, DMTF document DSP0214.
ModelCorrespondence | string | CIM_CLPProtocolEndpoint.OutputPosition
ValueMap | string | 2, 3, .., 0x8000..0xFFFF
Values | string | Begin, End, DMTF Reserved, Vendor Reserved
Write | boolean | true
OutputVerbosity | uint16 |
Description | string | OutputVerbosity establishes the default CLP Session output level of detail, as described in SM CLP Specification, DMTF document DSP0214.
ModelCorrespondence | string | CIM_CLPProtocolEndpoint.OutputVerbosity
ValueMap | string | 2, 3, 4, .., 0x8000..0xFFFF
Values | string | Error, Terse, Verbose, DMTF Reserved, Vendor Reserved
Write | boolean | true
WaitBehavior | boolean |
Description | string | When TRUE the CLP Session will not return a command response until all spawned jobs have completed, otherwise it may.
ModelCorrespondence | string | CIM_CLPProtocolEndpoint.WaitBehavior
Write | boolean | true

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
ChangeableType | uint16 | CIM_SettingData
ConfigurationName | string | CIM_SettingData
Description | string | CIM_ManagedElement
ElementName | string | CIM_SettingData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_SettingData
SoID | string | CIM_SettingData
SoOrgID | string | CIM_SettingData
ComponentSetting | string[] | CIM_SettingData

## Class Methods