# Class CIM_StoragePool
extends CIM_ResourcePool

A StoragePool is a conglomeration of storage capacity for the purpose of assignment and allocation based on service characteristics, such as location, available space or other criteria (for example, cost per megabyte or hardware ownership). A StoragePool is managed within the scope of a particular System. StoragePools may consist of component StoragePools or StorageExtents. StorageExtents that belong to the StoragePool have a Component relationship to the StoragePool. StorageExtents/StoragePools that are elements of a pool have their available space aggregated into the pool. StoragePools, StorageVolumes and LogicalDisks may be created from StoragePools. This is indicated by the AllocatedFromStoragePool association. StoragePool is scoped to a system by the HostedStoragePool association.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_ResourcePool
|
+--CIM_StoragePool

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | A StoragePool is a conglomeration of storage capacity for the purpose of assignment and allocation based on service characteristics, such as location, available space or other criteria (for example, cost per megabyte or hardware ownership). A StoragePool is managed within the scope of a particular System. StoragePools may consist of component StoragePools or StorageExtents. StorageExtents that belong to the StoragePool have a Component relationship to the StoragePool. StorageExtents/StoragePools that are elements of a pool have their available space aggregated into the pool. StoragePools, StorageVolumes and LogicalDisks may be created from StoragePools. This is indicated by the AllocatedFromStoragePool association. StoragePool is scoped to a system by the HostedStoragePool association.
UMLPackagePath | string | CIM::Device::StorageServices
Version | string | 2.49.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CapacityInMigratingSource | uint64 |
Description | string | The total capacity of extents in migrating out from this storage pool
Units | string | Bytes
CapacityInMigratingTarget | uint64 |
Description | string | The total capacity of extents in migrating into this storage pool
Units | string | Bytes
CompressionActive | boolean | false
Description | string | Indicates if the pool is compressed.
Experimental | boolean | true
CompressionPercent | uint8 |
Description | string | Indicates amount of compression on the pool.
Experimental | boolean | true
PUnit | string | Percent
CompressionRate | uint16 |
Description | string | CompressionRate identifies whether or not compression is being applied to the pool and at what rate.
Experimental | boolean | true
ValueMap | string | 0, 1, 2, 3, 4, .., 32768..65535
Values | string | Unknown, None, High, Medium, Low, DMTF Reserved, Vendor Specific
CompressionState | uint16 |
Description | string | The CompressionState indicates whether the compression is pending, initializing, in progress or completed.
Experimental | boolean | true
ValueMap | string | 1, 2, 3, 4, 5, .., 32768..65535
Values | string | Not applicable, Initializing, InProgress, Pending, Completed, DMTF Reserved, Vendor Specific
DedupActive | boolean | false
Description | string | Indicates if deduplication is active for this pool.
Experimental | boolean | true
DedupPercent | uint8 |
Description | string | Deduplication percentage of the pool.
Experimental | boolean | true
PUnit | string | Percent
ElementsShareSpace | boolean | false
Description | string | If true, it indicates elements allocated from the storage pool are sharing space from the storage pool. For example, multiple snapshots "allocated" from a storage pool, point to the same blocks of the storage pool. As another example, elements utilizing de-duplication technology refer to a shared copy of the data stored in the storage pool.
InstanceID | string |
Description | string | Within the scope of the instantiating Namespace, InstanceID opaquely and uniquely identifies an instance of this class. In order to ensure uniqueness within the NameSpace, the value of InstanceID SHOULD be constructed using the following 'preferred' algorithm: <OrgID>:<LocalID> Where <OrgID> and <LocalID> are separated by a colon ':', and where <OrgID> MUST include a copyrighted, trademarked or otherwise unique name that is owned by the business entity creating/defining the InstanceID, or is a registered ID that is assigned to the business entity by a recognized global authority (This is similar to the <Schema Name>_<Class Name> structure of Schema class names.) In addition, to ensure uniqueness <OrgID> MUST NOT contain a colon (':'). When using this algorithm, the first colon to appear in InstanceID MUST appear between <OrgID> and <LocalID>. <LocalID> is chosen by the business entity and SHOULD not be re-used to identify different underlying (real-world) elements. If the above 'preferred' algorithm is not used, the defining entity MUST assure that the resultant InstanceID is not re-used across any InstanceIDs produced by this or other providers for this instance's NameSpace. For DMTF defined instances, the 'preferred' algorithm MUST be used with the <OrgID> set to 'CIM'.
Key | boolean | true
Override | string | InstanceID
LowSpaceWarningThreshold | uint16 |
Description | string | LowSpaceWarningThreshold simplifies the creation of a pool specific Indication based on RemainingManagedSpace <= (TotalManagedSpace*LowSpaceWarningThreshold)/100. One example client for an Indication based on this property is a delta copy implementation where the pool enables continuous, variable space consumption for the delta storage. Another example client for an Indication based on this property is a provisioning manager implementing a policy for adding storage to a pool when it becomes low.
MaxValue | sint64 | 100
MinValue | sint64 | 0
ModelCorrespondence | string | CIM_StoragePool.RemainingManagedSpace
PUnit | string | percent
Units | string | Percentage
OtherUsageDescription | string |
Description | string | Populated when "Usage" has the value of "Other".
ModelCorrespondence | string | CIM_StoragePool.Usage
PoolID | string |
Description | string | A unique name in the context of the System that identifies this pool.
MaxLen | uint32 | 256
ModelCorrespondence | string | CIM_ResourceAllocationSettingData.PoolId
Override | string | PoolID
Required | boolean | true
Primordial | boolean | false
Description | string | If true, "Primordial" indicates that this StoragePool is the base from which storage capacity is drawn and returned in the activity of storage management. Being primordial means that this StoragePool shall not be created or deleted by consumers of this model. However, other actions, modeled or not, may affect the characteristics or size of primordial StoragePools. If false, "Primordial" indicated that the StoragePool, a concrete Storage Pool, is subject to storage services functions. This distinction is important because higher-level StoragePools may be assembled using the Component or AllocatedFromStoragePool associations. Although the higher-level abstractions can be created and deleted, the most basic, (i.e. primordial), hardware-based StoragePools cannot. They are physically realized as part of the System, or are actually managed by some other System and imported as if they were physically realized.
Override | string | Primordial
RemainingManagedSpace | uint64 |
Description | string | The remaining usable capacity after the allocation of StorageVolumes, LogicalDisks, or child Storage Pools. This property is maintained here to provide efficient access to this information. However, note that it is possible to compute RemainingManagedSpace as (TotalManagedSpace minus the sum of SpaceConsumed from all of the AllocatedFromStoragePool references from this StoragePool). Note that SpaceConsumed remains useful to determine the amount of capacity consumed by a particular allocated element.
ModelCorrespondence | string | CIM_StoragePool.TotalManagedSpace, CIM_AllocatedFromStoragePool.SpaceConsumed
PUnit | string | byte
Required | boolean | true
Units | string | Bytes
ReservedSpace | uint64 |
Description | string | The amount of capacity used by the storage pool to store information about the configuration of the storage pool. The space is not included in the TotalManagedSpace of the storage pool.
ModelCorrespondence | string | CIM_StoragePool.TotalManagedSpace
PUnit | string | byte
Units | string | Bytes
SpaceLimit | uint64 |
Description | string | The capacity of the storage allocated to the pool when SpaceLimitDetermination has the value 3 (Quota) or 4 (Limitless) or is set to the value of TotalManagedSpace if SpaceLimitDetermination has the value 2 (Allocated).
PUnit | string | byte
Units | string | Bytes
SpaceLimitDetermination | uint16 |
Description | string | This property is the Subsystem ID if the array or virtualizer supports Subsystem IDs. If they are supported they would be required on volume creation.
ValueMap | string | 2, 3, 4
Values | string | Allocated, Quote, Limitless
ThinProvisionMetaDataSpace | uint64 |
Description | string | The size of metadata consumed by this storage pool. Only defined if the pool is thin provisioned.
PUnit | string | byte
Units | string | Bytes
TotalManagedSpace | uint64 |
Description | string | The total amount of capacity usable for the allocation of StorageVolumes, LogicalDisks, or child Storage Pools. For primordial Storage Pools, this capacity reflects the usable capacity of Disk Drives or LUNs, for example, to the owning storage device or application. For example, in storage array, a primordial Storage Pool's TotalManagedSpace does not include metadata such as the disk label area and absolute disk drive capacity lost in disk formatting. For concrete Storage Pools, the same applies, but the metadata not included in TotalManagedSpace is consumed in virtualization like RAID and concatenation. Concrete Storage Pool may also be simple reserve of capacity. In such a case, no capacity may be lost in formation of the Storage Pool. Conceptually TotalManagedSpace is the sum of all storage known via AssociatedComponentExtent associations to underlying StorageExtents. However, note some of these underlying storage may not be modeled by the instrumentation.
ModelCorrespondence | string | CIM_StoragePool.RemainingManagedSpace
PUnit | string | byte
Units | string | Bytes
Usage | uint16 |
Description | string | Indicates the intended usage or any restrictions that may have been imposed on the usage of this component. For example, a storage pool may be reserved for use by the block server. In that case the Usage of the storage pool is marked as "Reserved for the ComputerSystem". In the case of "Other", see OtherUsageDescription for more information.
ModelCorrespondence | string | CIM_StoragePool.OtherUsageDescription
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, .., 32768..65535
Values | string | Other, Unrestricted, Reserved for ComputerSystem (the block server), Reserved as a Delta Replica Container, Reserved for Migration Services, Reserved for Local Replication Services, Reserved for Remote Replication Services, Reserved for Sparing, DMTF Reserved, Vendor Reserved
ClientSettableUsage | uint16[] |
Description | string | Indicates which values from the "Usage" valuemap can be manipulated by a client using the method "StorageConfigurationService.RequestUsageChange".
ModelCorrespondence | string | CIM_StoragePool.Usage

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AllocationUnits | string | CIM_ResourcePool
Capacity | uint64 | CIM_ResourcePool
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
ConsumedResourceUnits | string | CIM_ResourcePool
CurrentlyConsumedResource | uint64 | CIM_ResourcePool
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
MaxConsumableResource | uint64 | CIM_ResourcePool
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherResourceType | string | CIM_ResourcePool
PrimaryStatus | uint16 | CIM_ManagedSystemElement
Reserved | uint64 | CIM_ResourcePool
ResourceSubType | string | CIM_ResourcePool
ResourceType | uint16 | CIM_ResourcePool
Status | string | CIM_ManagedSystemElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Local Class Methods

#### GetSupportedSizes (uint32)

#### Method Qualifiers (GetSupportedSizes)

Name | Data Type | Value
--- | --- | ---
Description | string | For pools that that support a range of sizes for volume or pool creation, this method can be used to retrieve the supported range. Note that different pool implementations may support either or both the GetSupportedSizes and GetSupportedSizeRanges methods at different times, depending on Pool configuration. Also note that the advertised sizes may change after the call due to requests from other clients. If the pool currently only supports discrete sizes, then the return value will be set to 1.
ValueMap | string | 0, 1, 2, 3
Values | string | Method completed OK, Method not supported, Use GetSupportedSizeRange instead, Invalid Element Type

#### Method Parameters (GetSupportedSizes)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
ElementType | uint16
Description | string | The type of element for which supported sizes are reported. The Thin Provision values are only supported when the Thin Provisioning Profile is supported; the resulting StorageVolume/LogicalDisk shall have ThinlyProvisioned set to true.
ValueMap | string | 2, 3, 4, 5, 6
Values | string | Storage Pool, Storage Volume, Logical Disk, Thin Provisioned Volume, Thin Provisioned Logical Disk
Sizes | uint64[]
Description | string | List of supported sizes for a Volume/Pool creation or modification.
OUT | boolean | true
PUnit | string | byte
Units | string | Bytes
Goal | REF CIM_StorageSetting
Description | string | The StorageSetting for which supported sizes should be reported for.

#### GetSupportedSizeRange (uint32)

#### Method Qualifiers (GetSupportedSizeRange)

Name | Data Type | Value
--- | --- | ---
Description | string | For pools that that support a range of sizes for volume or pool creation, this method can be used to retrieve the supported range. Note that different pool implementations may support either or both the GetSupportedSizes and GetSupportedSizeRanges methods at different times, depending on Pool configuration. Also note that the advertised sizes may change after the call due to requests from other clients. If the pool currently only supports discrete sizes, then the return value will be set to 1.
ValueMap | string | 0, 1, 2, 3
Values | string | Method completed OK, Method not supported, Use GetSupportedSizes instead, Invalid Element Type

#### Method Parameters (GetSupportedSizeRange)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
ElementType | uint16
Description | string | The type of element for which supported size ranges are reported. The Thin Provision values are only supported when the Thin Provisioning Profile is supported; the resulting StorageVolume/LogicalDisk shall have ThinlyProvisioned set to true.
ValueMap | string | 2, 3, 4, 5, 6
Values | string | Storage Pool, Storage Volume, Logical Disk, Thin Provisioned Volume, Thin Provisioned Logical Disk
MaximumVolumeSize | uint64
Description | string | The maximum size for a volume/pool in bytes.
OUT | boolean | true
PUnit | string | byte
Units | string | Bytes
MinimumVolumeSize | uint64
Description | string | The minimum size for a volume/pool in bytes.
OUT | boolean | true
PUnit | string | byte
Units | string | Bytes
VolumeSizeDivisor | uint64
Description | string | A volume/pool size must be a multiple of this value which is specified in bytes.
OUT | boolean | true
PUnit | string | byte
Units | string | Bytes
Goal | REF CIM_StorageSetting
Description | string | The StorageSetting for which supported size ranges should be reported for.

#### GetAvailableExtents (uint32)

#### Method Qualifiers (GetAvailableExtents)

Name | Data Type | Value
--- | --- | ---
Description | string | This method can be used to retrieve a list of available Extents that may be used in the creation or modification of a StoragePool, StorageVolume, or LogicalDisk. The GetAvailableExtents method MUST return the Extents from the set of Component Extents of the Pool on which the method is being invoked. The returned Extents are available at the time the method returns. There is no guarantee that the same Extents will be available later. This method MUST return the Extents that are not being used as supporting capacity for any other Pools, Volumes, or LogicalDisks that have been allocated from this Pool. The Extent returned MUST be a component Extent of the Pool or subdivisions of a component Extent, the subdivisions themselves represented as Extents.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4098..32767, 32768..65535
Values | string | Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Reserved, Vendor Specific

#### Method Parameters (GetAvailableExtents)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
AvailableExtents | CIM_StorageExtent[]
Description | string | List of references to available StorageExtents, or subclass instances.
OUT | boolean | true
Goal | REF CIM_StorageSetting
Description | string | The StorageSetting (Goal) for which supported extents should be retrieved as available. If a NULL is passed for the Goal, the method will return all available extents, regardless of the goal. There exists a possibility of error in creating a Pool, Volume, or LogicalDisk retrieved in this manner.